InS_StArT
TCNSW.COM
1.0
^Thomas-Conrad TC3042 TCNS 8-bit adapter,TCNSW.COM,IE0
^Thomas-Conrad TC3045 TCNS 16-bit adapter,TCNSW.COM,IE0
^Thomas-Conrad TC3046 TCNS MC adapter,TCNSW.COM,00M,64B7
^Thomas-Conrad TC3047 TCNS EISA adapter,TCNSW.COM,0E0,TCO3147
?Select the options that match your adapter's settings. Your adapter must be in Enhanced mode.
!RIE0(INT) Hardware Interrupt
@2
3
4
5
6
7
9
10
11
12
14
15
!RIE0(MEM) Base Memory Address
C0000
C4000
C8000
CC000
@D0000
D4000
D8000
DC000
!O00M(SLOT) Slot
?If a slot is not selected, the driver will check the configuration for a slot number.
1
2
3
4
5
6
7
8
$OIEM(MAX FRAME SIZE) Maximum Frame Size
?Select Maximum Frame Size.  Default: 4216.  Larger frame sizes may improve performance.
618
16490
InS_EnD
