InS_StArT
TPROODI.COM
1.0
^Intel TokenExpress(TM) PRO Adapter,TPROODI.COM,IE0
?The driver can communicate across Source Routing bridges. To enable this, load the ROUTE.COM module after TPROODI.COM
!OIE0(PORT)Base I/O Port
?If more than one TokenExpress PRO Adapter is installed in the workstation, use the PORT parameter to identify the adapter.
300
310
320
330
340
350
360
$OIE0(NODE ADDRESS)
400000000000
7FFFFFFFFFFF
*OIE0(FRAME)
?Select the frame type(s) used by the protocols in the workstation. If no frame type(s) is specified, TOKEN-RING MSB will be supported. The LSB and MSB attributes are mutually exclusive and should not both be selected for the same frame type.
TOKEN-RING MSB
TOKEN-RING LSB
TOKEN-RING_SNAP MSB
TOKEN-RING_SNAP LSB
InS_EnD

