InS_StArT
TCE32ESW.COM
1.0
^Thomas-Conrad TC5047 Ethernet adapter,TCE32ESW.COM,IE0
!R0E0(SLOT) Slot 
?Select the slot number that corresponds to the expansion slot where the board is installed.
0
1
2
3
4
5
6
7
8
9
a
b
c
e
d
f
*OIE0(FRAME) Frame Type
@Ethernet_802.2
Ethernet_II
Ethernet_802.3
Ethernet_SNAP
$OIE0(NODE ADDRESS) Node Address
?Select none unless you want to set a locally administered Node ID in the range shown below.
008013000000
008013FFFFFF
InS_EnD
